# There are a number of modifiers that are allowed to be used in some
# of the different fields. They provide the following subsitutions:
#
# %n the "kernel number" of the device.
#    For example, 'sda3' has a "kernel number" of '3'
# %e the smallest number for that name which does not matches an existing node
# %k the kernel name for the device
# %M the kernel major number for the device
# %m the kernel minor number for the device
# %b the bus id for the device
# %c the string returned by the PROGRAM
# %s{filename} the content of a sysfs attribute
# %% the '%' char itself
#

# Media automounting
SUBSYSTEM=="block", ACTION=="add"    RUN+="/etc/udev/scripts/mount.sh"
SUBSYSTEM=="block", ACTION=="remove" RUN+="/etc/udev/scripts/mount.sh"

# Handle network interface setup
SUBSYSTEM=="net", ACTION=="add" RUN+="/etc/udev/scripts/network.sh"
SUBSYSTEM=="net", ACTION=="remove" RUN+="/etc/udev/scripts/network.sh"

# The first framebuffer is symlinked to /dev/fb                       
KERNEL=="fb0", SYMLINK+="fb"

# The first rtc device is symlinked to /dev/rtc
KERNEL=="rtc0", SYMLINK+="rtc"

# Try and modprobe for drivers for new hardware
ACTION=="add", DEVPATH=="/devices/*", ENV{MODALIAS}=="?*", RUN+="/sbin/modprobe $env{MODALIAS}"

# Create a symlink to any touchscreen input device
SUBSYSTEM=="input", KERNEL=="event[0-9]*", ATTRS{modalias}=="input:*-e0*,3,*a0,1,*18,*", SYMLINK+="input/touchscreen0"

