# gsmd	This shell script configures for the gsmd init script.

. /etc/init.d/functions

case `cpuinfo_id` in
	"GTA01"|"GTA02")
		GSMD_OPTS="-s 115200 -F"
		GSM_POW="/sys/bus/platform/devices/gta01-pm-gsm.0/power_on"
		GSM_RES="/sys/bus/platform/devices/gta01-pm-gsm.0/reset"
		GSM_DEV="/dev/ttySAC0"
		;;
	"HTC Apache"|"HTC Blueangel"|"HTC Universal")
		GSMD_OPTS="-s 115200 -F"
		GSM_DEV="/dev/ttyS0"
		;;
	"HTC Himalaya")
		GSMD_OPTS="-s 115200 -F"
		GSM_DEV="/dev/ttyS2"
		;;
	"HTC Magician")
		GSMD_OPTS="-s 115200 -F"
		GSM_DEV="/dev/ttyS1"
		;;
	"Palm Treo 650")
		GSMD_OPTS="-s 460800 -F -w 1"
		GSM_DEV="/dev/ttyS0"
		;;
        "Motorola Ezx Platform")
                GSMD_OPTS="-s 115200 -F -v ti"
                GSM_DEV="/dev/mux0"
                ;;
	*)
		# Unknown board

		# If you must specify special options, uncomment and modify the next line
		#GSMD_OPTS="-s 115200 -F"

		# If your GSM device needs to be powered up, uncomment and modify the next line
		#GSM_POW="/sys/bus/platform/devices/gta01-pm-gsm.0/power_on"

		# If your GSM device then needs to be reset, uncomment and modify the next line
		#GSM_RES="/sys/bus/platform/devices/gta01-pm-gsm.0/reset"

		# This should be in a common /etc/default/serial, together with
		# BT_DEV and IR_DEV for devices that have those on a serial port
		#GSM_DEV="/dev/ttyS1"
		;;
esac
