require linux-rp.inc

PR = "r10"

DEFAULT_PREFERENCE_collie = "1"

# Handy URLs
# git://git.kernel.org/pub/scm/linux/kernel/git/torvalds/linux-2.6.git;protocol=git;tag=ef7d1b244fa6c94fb76d5f787b8629df64ea4046
# ${KERNELORG_MIRROR}pub/linux/kernel/v2.6/linux-2.6.18.tar.bz2
# ${KERNELORG_MIRROR}pub/linux/kernel/v2.6/testing/linux-2.6.20-rc4.tar.bz2
# ${KERNELORG_MIRROR}pub/linux/kernel/v2.6/testing/patch-2.6.18-rc6.bz2;patch=1
# ${KERNELORG_MIRROR}pub/linux/kernel/v2.6/snapshots/patch-2.6.18-rc2-git1.bz2;patch=1
# ${KERNELORG_MIRROR}pub/linux/kernel/people/alan/linux-2.6/2.6.10/patch-2.6.10-ac8.gz;patch=1
# ${KERNELORG_MIRROR}pub/linux/kernel/people/akpm/patches/2.6/2.6.14-rc2/2.6.14-rc2-mm1/2.6.14-rc2-mm1.bz2;patch=1

# Patches submitted upstream are towards top of this list 
# Hacks should clearly named and at the bottom
SRC_URI = "${KERNELORG_MIRROR}pub/linux/kernel/v2.6/linux-2.6.21.tar.bz2 \
           ${RPSRC}/lzo_kernel-r0.patch;patch=1 \
           ${RPSRC}/lzo_jffs2-r0.patch;patch=1 \
           ${RPSRC}/lzo_crypto-r1.patch;patch=1 \
           ${RPSRC}/lzo_jffs2_lzomode-r0.patch;patch=1 \
           ${RPSRC}/lzo_jffs2_sysfs-r0.patch;patch=1 \
           ${RPSRC}/hx2750_base-r28.patch;patch=1 \
           ${RPSRC}/hx2750_bl-r9.patch;patch=1 \
           ${RPSRC}/hx2750_pcmcia-r2.patch;patch=1 \
           ${RPSRC}/pxa_keys-r7.patch;patch=1 \
           ${RPSRC}/tsc2101-r16.patch;patch=1 \
           ${RPSRC}/hx2750_test1-r6.patch;patch=1 \
           ${RPSRC}/pxa_timerfix-r0.patch;patch=1 \
           ${RPSRC}/input_power-r7.patch;patch=1 \
           ${RPSRC}/pxa25x_cpufreq-r2.patch;patch=1 \
           ${RPSRC}/sharpsl_pm_fixes1-r0.patch;patch=1 \
           ${RPSRC}/pm_changes-r1.patch;patch=1 \
           ${RPSRC}/usb_add_epalloc-r3.patch;patch=1 \
           ${RPSRC}/usb_pxa27x_udc-r4.patch;patch=1 \
           ${RPSRC}/locomo_kbd_tweak-r1.patch;patch=1 \
           ${RPSRC}/poodle_pm-r4.patch;patch=1 \
           ${RPSRC}/pxa27x_overlay-r5.patch;patch=1 \
           ${RPSRC}/w100_extaccel-r0.patch;patch=1 \
           ${RPSRC}/asoc_fix_typo-r0.patch;patch=1 \
           ${RPSRC}/qemuarm_scsi_fix-r0.patch;patch=1 \
           file://hostap-monitor-mode.patch;patch=1 \
           file://serial-add-support-for-non-standard-xtals-to-16c950-driver.patch;patch=1 \
           ${RPSRC}/logo_oh-r0.patch.bz2;patch=1;status=unmergable \
           ${RPSRC}/logo_oz-r2.patch.bz2;patch=1;status=unmergable \
           ${RPSRC}/pxa-linking-bug.patch;patch=1;status=unmergable \
           ${RPSRC}/mmcsd_large_cards-r0.patch;patch=1;status=hack \
           ${RPSRC}/mmcsd_no_scr_check-r0.patch;patch=1;status=hack \
           ${RPSRC}/integrator_rgb-r1.patch;patch=1;status=hack \
           ${RPSRC}/pxa_cf_initorder_hack-r1.patch;patch=1;status=hack \
           file://pxa-serial-hack.patch;patch=1;status=hack \
           file://connectplus-remove-ide-HACK.patch;patch=1;status=hack \
	   file://connectplus-prevent-oops-HACK.patch;patch=1;status=hack \
           file://squashfs3.0-2.6.15.patch;patch=1;status=external \
           file://vesafb-tng-1.0-rc2-2.6.20-rc2.patch;patch=1;status=external \
           file://sharpsl-rc-r1.patch;patch=1 \
           file://defconfig-c7x0 \
           file://defconfig-hx2000 \
           file://defconfig-collie \
           file://defconfig-poodle \
           file://defconfig-akita \
           file://defconfig-spitz \
           file://defconfig-qemuarm \
           file://defconfig-qemux86 \
           file://defconfig-bootcdx86 \
           file://defconfig-tosa "

# Add this to enable pm debug code (useful with a serial lead)
#  ${RPSRC}/sharpsl_pm_debug-r0.patch;patch=1

# Disabled until I find the reason this gives issues with cdc_subset
#            ${RPSRC}/usb_rndis_tweaks-r0.patch;patch=1 \

# Is anything out of this still needed? Parts were commited to mainline by rmk (drivers/mfd/)
# (Pavel Machek's git tree has updated versions of this?)
#  ${JLSRC}/zaurus-lcd-2.6.11.diff.gz;patch=1

SRC_URI_append_collie = "\
 	   ${TKSRC}/mtd-sharp-flash-hack-r2.patch;patch=1 \
           ${TKSRC}/ucb1x00-touch-audio-r1.patch;patch=1 \
 	   ${TKSRC}/mcp-sa11x0-r0.patch;patch=1 \
 	   ${TKSRC}/sa1100-udc-r2.patch;patch=1 \
 	   ${TKSRC}/mmc_spi-r4.patch;patch=1 \
 	   ${TKSRC}/locomo-r0.patch;patch=1 \
 	   ${TKSRC}/collie-kexec.patch;patch=1 \
 	   ${TKSRC}/locomo_spi-r4.patch;patch=1 \
 	   ${TKSRC}/sharpsl_pm-r2.patch;patch=1 \
 	   ${TKSRC}/collie_pm-r2.patch;patch=1 \
 	   ${TKSRC}/locomokeyb_suspendkey-2.patch;patch=1 \
 	   ${TKSRC}/pcmcia_suspend.patch;patch=1 \
 	   ${TKSRC}/ucb1x00_suspend.patch;patch=1 \
"

SRC_URI_append_tosa = "\
           ${CHSRC}/usb-ohci-hooks-r1.patch;patch=1 \
           ${CHSRC}/tmio-core-r4.patch;patch=1 \
           file://tmio-tc6393-r8.patch;patch=1 \
           file://tmio-nand-r7.patch;patch=1 \
           file://tmio-ohci-r6.patch;patch=1 \
           ${CHSRC}/tmio-fb-r6.patch;patch=1 \
           file://tosa-keyboard-r18.patch;patch=1 \
           ${DOSRC}/tosa-pxaac97-r6.patch;patch=1 \
           ${DOSRC}/tosa-tmio-r6.patch;patch=1 \
           ${DOSRC}/tosa-power-r17.patch;patch=1 \
           file://tosa-tmio-lcd-r10.patch;patch=1 \
           ${DOSRC}/tosa-bluetooth-r8.patch;patch=1 \
           ${DOSRC}/wm97xx-lg7-r0.patch;patch=1 \
           file://wm9712-suspend-cold-res-r2.patch;patch=1 \
           file://sharpsl-pm-postresume-r1.patch;patch=1 \
           ${DOSRC}/wm97xx-dig-restore-r0.patch;patch=1 \
           ${DOSRC}/wm97xx-miscdevs-resume-r0.patch;patch=1 \
           file://wm9712-reset-loop-r2.patch;patch=1 \
           file://tosa-lcdnoise-r1.patch;patch=1 \
           file://wm97xx-lcdnoise-r0.patch;patch=1 "
#          ${DOSRC}/tosa-asoc-r1.patch;patch=1 "

S = "${WORKDIR}/linux-2.6.21"
