#!/bin/sh
#
# H3600 Sleeve hotplug policy agent for Linux 2.4 kernels
#
# Kernel NET hotplug params include:
#	
#	ACTION=%s [add or remove]
#	MEDIA=%s
#	SLOT=%d
#

. /etc/hotplug/hotplug.functions
#DEBUG=yes export DEBUG

    echo "Executing $0 action=$ACTION, media=$MEDIA ($SLOT)" > /dev/console

MMC_MOUNT_OPTIONS="-t auto -o sync,noatime"

if [ -f /etc/sysconfig/hotplug ] ; then
    . /etc/sysconfig/hotplug
fi

case `uname -r` in
2.4*)
    devpath=mmc/part
    ;;
*)
    devpath=mmcblk0p
    ;;
esac

if [ "$ACTION" = "add" ] ; then
    sleep 4
    echo -n add > /dev/console
    for n in 1 2 3 4 ; do
	device=/dev/$devpath$n
	if [ "$n" = "1" ] ; then
	    card=/mnt/card
	else
	    card=/mnt/card$n
	fi
	[ -b $device ] || break
	echo " flash on $device" > /dev/console
	[ -d $card ] || mkdir -p $card
	mount $MMC_MOUNT_OPTIONS $device $card
    done

else
    for card in /mnt/card*; do
	umount $card
    done
fi
