From e7d6e37675e422cfab2fe8c6bd411d2097228760 Mon Sep 17 00:00:00 2001
From: Yuval Shaia <yuval.shaia.ml@gmail.com>
Date: Wed, 1 Mar 2023 16:29:26 +0200
Subject: [PATCH] hw/pvrdma: Protect against buggy or malicious guest driver

Guest driver allocates and initialize page tables to be used as a ring
of descriptors for CQ and async events.
The page table that represents the ring, along with the number of pages
in the page table is passed to the device.
Currently our device supports only one page table for a ring.

Let's make sure that the number of page table entries the driver
reports, do not exceeds the one page table size.

CVE: CVE-2023-1544
Upstream-Status: Backport [https://gitlab.com/qemu-project/qemu/-/commit/85fc35afa93c]

Reported-by: Soul Chen <soulchen8650@gmail.com>
Signed-off-by: Yuval Shaia <yuval.shaia.ml@gmail.com>
Fixes: CVE-2023-1544
Message-ID: <20230301142926.18686-1-yuval.shaia.ml@gmail.com>
Signed-off-by: Thomas Huth <thuth@redhat.com>
(cherry picked from commit 85fc35afa93c7320d1641d344d0c5dfbe341d087)
Signed-off-by: Niranjan Pradhan <nirpradh@cisco.com>
---
 hw/rdma/vmw/pvrdma_main.c | 16 +++++++++++++++-
 1 file changed, 15 insertions(+), 1 deletion(-)

diff --git a/hw/rdma/vmw/pvrdma_main.c b/hw/rdma/vmw/pvrdma_main.c
index 4fc6712025..55b338046e 100644
--- a/hw/rdma/vmw/pvrdma_main.c
+++ b/hw/rdma/vmw/pvrdma_main.c
@@ -91,19 +91,33 @@ static int init_dev_ring(PvrdmaRing *ring, PvrdmaRingState **ring_state,
                          dma_addr_t dir_addr, uint32_t num_pages)
 {
     uint64_t *dir, *tbl;
-    int rc = 0;
+    int max_pages, rc = 0;
 
     if (!num_pages) {
         rdma_error_report("Ring pages count must be strictly positive");
         return -EINVAL;
     }
 
+    /*
+     * Make sure we can satisfy the requested number of pages in a single
+     * TARGET_PAGE_SIZE sized page table (taking into account that first entry
+     * is reserved for ring-state)
+     */
+    max_pages = TARGET_PAGE_SIZE / sizeof(dma_addr_t) - 1;
+    if (num_pages > max_pages) {
+        rdma_error_report("Maximum pages on a single directory must not exceed %d\n",
+                          max_pages);
+        return -EINVAL;
+    }
+
     dir = rdma_pci_dma_map(pci_dev, dir_addr, TARGET_PAGE_SIZE);
     if (!dir) {
         rdma_error_report("Failed to map to page directory (ring %s)", name);
         rc = -ENOMEM;
         goto out;
     }
+
+    /* We support only one page table for a ring */
     tbl = rdma_pci_dma_map(pci_dev, dir[0], TARGET_PAGE_SIZE);
     if (!tbl) {
         rdma_error_report("Failed to map to page table (ring %s)", name);
-- 
2.35.6

