#!/bin/sh
#
# Devfs handling script.  Since we arent running devfsd due to various reasons
# which I will not lay out here, we need to create some links for compatibility.

# exit without doing anything if udev is active
if test -e /dev/.udevdb; then
    exit 0
fi

    test -n "$VERBOSE" && echo -n "Setting up device links for devfs: "
    (
    ln -s /dev/vc/0 /dev/tty0
    ln -s /dev/vc/1 /dev/tty1
    ln -s /dev/vc/2 /dev/tty2
    ln -s /dev/vc/3 /dev/tty3
    ln -s /dev/vc/4 /dev/tty4
    ln -s /dev/vc/5 /dev/tty5
    ln -s /dev/fb/0 /dev/fb0
    # ln -s /dev/tts/0 /dev/ttySA0
    # ln -s /dev/tts/1 /dev/ttySA1
    # ln -s /dev/tts/2 /dev/ttySA2

    ln -s /dev/sound/dsp /dev/dsp
    ln -s /dev/sound/mixer /dev/mixer

    ln -s /dev/v4l/video0 /dev/video0
    ln -s /dev/v4l/video0 /dev/video
    ln -s /dev/misc/rtc /dev/rtc
    ln -s /dev/misc/apm_bios /dev/apm_bios

    ## need this so that ppp will autoload the ppp modules
    mknod /dev/ppp c 108 0
    )  > /dev/null 2>&1


    test -n "$VERBOSE" && echo "done"
