Platform: Sharp Zaurus C760 running 2.6.16 and pcmciautils 013.

root@c7x0:~# pccardctl ident
Socket 0:
  product info: "Pretec", "CompactWLAN Card 802.11b", "2.5"
  manfid: 0x0156, 0x0002
  function: 6 (network)

==========================================================================
From: Jochen Friedrich 

Yet another card known to work OK with hostap_cs:

# pccardctl ident
Socket 0:
  no product info available
Socket 1:
  product info: "U.S. Robotics", "IEEE 802.11b PC-CARD", "Version 01.02", ""
  manfid: 0x0156, 0x0002
  function: 6 (network)

==========================================================================

Signed-off-by: Marcin Juszkiewicz <openembedded@hrw.one.pl>

 drivers/net/wireless/hostap/hostap_cs.c |    6 ++++++
 1 file changed, 6 insertions(+)

Index: linux/drivers/net/wireless/hostap/hostap_cs.c
===================================================================
--- linux.orig/drivers/net/wireless/hostap/hostap_cs.c	2006-05-17 10:23:00.000000000 +0200
+++ linux/drivers/net/wireless/hostap/hostap_cs.c	2006-05-17 10:25:45.000000000 +0200
@@ -923,6 +923,12 @@
 	PCMCIA_DEVICE_PROD_ID12(
 		"ZoomAir 11Mbps High", "Rate wireless Networking",
 		0x273fe3db, 0x32a1eaee),
+	PCMCIA_DEVICE_PROD_ID123(
+			"Pretec", "CompactWLAN Card 802.11b", "2.5",
+			0x1cadd3e5, 0xe697636c, 0x7a5bfcf1),
+	PCMCIA_DEVICE_PROD_ID123(
+		"U.S. Robotics", "IEEE 802.11b PC-CARD", "Version 01.02",
+		0xc7b8df9d, 0x1700d087, 0x4b74baa0),
 	PCMCIA_DEVICE_NULL
 };
 MODULE_DEVICE_TABLE(pcmcia, hostap_cs_ids);
