#!/bin/sh

# Handle running Poky images under qemu
#
# Copyright (C) 2006-2007 OpenedHand Ltd.
#
# This program is free software; you can redistribute it and/or modify
# it under the terms of the GNU General Public License version 2 as
# published by the Free Software Foundation.
#
# This program is distributed in the hope that it will be useful,
# but WITHOUT ANY WARRANTY; without even the implied warranty of
# MERCHANTABILITY or FITNESS FOR A PARTICULAR PURPOSE.  See the
# GNU General Public License for more details.
#
# You should have received a copy of the GNU General Public License along
# with this program; if not, write to the Free Software Foundation, Inc.,
# 51 Franklin Street, Fifth Floor, Boston, MA 02110-1301 USA.


# Call setting:
#   QEMU_MEMORY (optional) set the amount of memory in the emualted system.
#   SERIAL_LOGFILE (optional) log the serial port output to a file
#
# Image options:
#   MACHINE - the machine to run
#   TYPE - the image type to run
#   ZIMAGE - the kernel image file to use
#   HDIMAGE - the disk image file to use
#

QEMUIFUP=`which poky-qemu-ifup`
KERNEL_NETWORK_CMD="ip=192.168.7.2::192.168.7.1:255.255.255.0"
QEMU_NETWORK_CMD="-net nic,vlan=0 -net tap,vlan=0,ifname=tap0,script=$QEMUIFUP"

if [ -z "$QEMU_MEMORY" ]; then
    QEMU_MEMORY="64M"
fi

SERIALOPTS=""
if [ "x$SERIAL_LOGFILE" != "x" ]; then
    SERIALOPTS="-serial file:$SERIAL_LOGFILE"
fi

if [ "$TYPE" != "nfs" -a ! -f "$HDIMAGE" ]; then
    echo "Error, image file $HDIMAGE doesn't exist"
    return
fi

if [ ! -f "$ZIMAGE" ]; then
    echo "Error, kernel image file $ZIMAGE doesn't exist"
    return
fi

if [ "$MACHINE" != "qemuarm" -a "$MACHINE" != "qemux86" -a "$MACHINE" != "akita" -a "$MACHINE" != "spitz" ]; then
    echo "Error, unsupported machine type $MACHINE"
    return
fi

if [ "$MACHINE" = "qemuarm" ]; then
    QEMU=`which qemu-system-arm`
    if [ "$TYPE" = "ext2" ]; then
        QEMUOPTIONS="-append \"root=/dev/sda console=ttyAMA0 console=tty0 mem=$QEMU_MEMORY\" $QEMU_NETWORK_CMD -M versatilepb -hda $HDIMAGE -usb -usbdevice wacom-tablet"
    fi
    if [ "$TYPE" = "nfs" ]; then
        if [ "x$HDIMAGE" = "x" ]; then
            HDIMAGE=/srv/nfs/qemuarm
        fi
        if [ ! -d "$HDIMAGE" ]; then
            echo "Error, NFS mount point $HDIMAGE doesn't exist"
            return
        fi
        QEMUOPTIONS="-append \"root=/dev/nfs nfsroot=192.168.7.1:$HDIMAGE rw $KERNEL_NETWORK_CMD\" $QEMU_NETWORK_CMD -M versatilepb"
    fi
fi

if [ "$MACHINE" = "qemux86" ]; then
    QEMU=`which qemu`
    if [ "$TYPE" = "ext2" ]; then
        QEMUOPTIONS="-std-vga -append \"root=/dev/hda mem=$QEMU_MEMORY $KERNEL_NETWORK_CMD\" $QEMU_NETWORK_CMD -hda $HDIMAGE -usb -usbdevice wacom-tablet"
    fi
    if [ "$TYPE" = "nfs" ]; then
        if [ "x$HDIMAGE" = "x" ]; then
            HDIMAGE=/srv/nfs/qemux86
        fi
        if [ ! -d "$HDIMAGE" ]; then
            echo "Error, NFS mount point $HDIMAGE doesn't exist."
            return
        fi
        QEMUOPTIONS="-std-vga -append \"root=/dev/nfs nfsroot=192.168.7.1:$HDIMAGE rw $KERNEL_NETWORK_CMD\" $QEMU_NETWORK_CMD"
    fi
fi

if [ "$MACHINE" = "spitz" ]; then
    QEMU=`which qemu-system-arm`
    if [ "$TYPE" = "ext3" ]; then
        echo $HDIMAGE
        HDIMAGE=`readlink -f $HDIMAGE`
        echo $HDIMAGE
        if [ ! -e "$HDIMAGE.qemudisk" ]; then
            echo "Adding a partition table to the ext3 image for use by QEMU, please wait..."
            poky-addptable2image $HDIMAGE $HDIMAGE.qemudisk
        fi
        QEMUOPTIONS="$QEMU_NETWORK_CMD -M spitz -hda $HDIMAGE.qemudisk -portrait"
    fi
fi

if [ "$MACHINE" = "akita" ]; then
    QEMU=`which qemu-system-arm`
    if [ "$TYPE" = "jffs2" ]; then
        HDIMAGE=`readlink -f $HDIMAGE`
        if [ ! -e "$HDIMAGE.qemuflash" ]; then
            echo "Converting raw image into flash image format for use by QEMU, please wait..."
	    raw2flash.akita < $HDIMAGE > $HDIMAGE.qemuflash
        fi
        QEMUOPTIONS="$QEMU_NETWORK_CMD -M akita -mtdblock $HDIMAGE.qemuflash -portrait"
    fi
fi

if [ "x$QEMUOPTIONS" = "x" ]; then
    echo "Error, unable to support this combination of options"
    return
fi

echo "Running $QEMU using sudo..."
echo "$QEMU -kernel $ZIMAGE $QEMUOPTIONS $SERIALOPTS"
sudo $QEMU -kernel $ZIMAGE $QEMUOPTIONS $SERIALOPTS


